**Gill Athletics, Inc.**

**F44124 – READY-FIT ALUMINUM SAND PIT COVER; 24’**

**SECTION 11 68 33.43**

**READY-FIT ALUMINUM SAND PIT COVER**

**PART 1 GENERAL**

**1.01 SECTION INCLUDES**

A. ALUMINUM SAND PIT COVER

**1.02 RELATED SECTIONS**

A. Section 31 23 00 Excavation and Fill.

B. Section 03 30 00 Cast-in-Place Concrete.

C. Section 32 18 23 Athletic Surfacing.

D. Section 32 12 16 Asphalt Paving.

**1.03 REFERENCES**

1. NFHS – National Federation of State High School Associations (NFHS)
2. NCAA – National Collegiate Athletic Association (NCAA)
3. IAAF – International Association of Athletics Federations (IAAF)
4. FIFA – International Federation of Association Football
5. FIBA – International Basketball Federation

**1.04 DESIGN REQUIREMENTS**

1. Sand Pit Cover: Locate position of sand pit cover on the site plan.
2. Verify that site conditions are adequate to support loads imposed by sand pit cover.

**1.05 SUBMITTALS**

1. Comply with Section 01 33 00 – Submittal Procedures.
2. Product Data: Submit manufacturer's product data, including materials, components, fabrication, finish, and installation instructions.
3. Operation and Maintenance Manual: Submit manufacturer's operation and maintenance manual; including operation, maintenance, adjustment, and cleaning instructions; trouble shooting guide; parts list.

**1.06 QUALITY ASSURANCE**

A. Single Source Responsibility: Provide sand pit cover from single manufacturer.

B. Manufacturer's Qualifications: Minimum of 5 consecutive years of experience manufacturing sand pit covers similar to that specified.

C. Installer's Qualifications: Contractor experienced with track & field installation, concrete work, asphalt paving, and track surfacing.

D. Regulatory Requirements: Sand pit cover shall conform to latest rules and regulations.

1. National Federation of State High School Associations (NFHS).

2. National Collegiate Athletic Association (NCAA)

3. International Association of Athletics Federations (IAAF)

4. International Federation of Association Football (FIFA)

5. International Basketball Federation (FIBA)

**1.07 DELIVERY, STORAGE, AND HANDLING**

A. Delivery: Deliver materials to site in manufacturer's original, unopened containers and packaging, with labels clearly identifying product name and manufacturer.

B. Storage: Store materials in clean, dry area indoors in accordance with manufacturer's instructions. Keep temporary protective coverings in place.

C. Handling: Protect materials and finish from damage during handling and installation.

**1.08 WARRANTY**

A. Provide 1-year warranty against defects in materials and workmanship, unless otherwise specified.

**PART 2 PRODUCTS**

**2.01 MANUFACTURER**

A. Manufactured and Supplied by:

 Gill Athletics, Inc.

 601 Mercury Drive

 Champaign, Illinois 61822

 Toll Free (800) 637-3090

 Phone (217) 367-8438

 Fax (217) 367-8440

 Web Site [www.gillathletics.com](http://www.gillathletics.com)

 E-Mail sales@gillathletics.com

**2.02 F44124 – READY-FIT ALUMINUM SAND PIT COVER; 24’**

1. COMPONENTS:
2. Cover
	1. Consists of ten (10) covers
	2. 28 15/16” W x 115 1/2" L
	3. Each Cover is constructed of three (3) Aluminum Panels
	4. Recessed to receive synthetic track surface
	5. End Angles
		1. Aluminum
		2. 1-1/2" W x 2-3/8” H x 3/16”
		3. Welded on the outer walls of panels
3. Flat Bar
	1. Aluminum
	2. 2-1/2” W x 3/16”
	3. Welded to the Underside of Covers
4. Handles
	1. Zinc Coated Steel
	2. 4” W x 3” H x 1/2"
	3. 4 per Panel

**PART 3 EXECUTION**

**3.01 EXAMINATION**

A. Examine area to receive sand pit cover. Notify Architect in writing of conditions that would adversely affect installation or subsequent use. Do not proceed with installation until unsatisfactory conditions are corrected.

**3.02 INSTALLATION**

A. Install sand pit cover in accordance with manufacturer's instructions at locations indicated on the Drawings.

B. Install equipment plumb, level, straight, square, accurately aligned, correctly located, to proper elevation, and secure.

C. Install equipment using manufacturer's supplied hardware and fasteners.

D. Repair minor damages to finish in accordance with manufacturer's instructions and as approved by Architect.

1. Remove and replace damaged components that cannot be successfully repaired, as determined by Architect.

**3.03 ADJUSTING**

1. Adjust product name to plumb and level as appropriate.

 **END OF SECTION**